Improvements with this firmware:

1. Rectified the bug that unexpected gaps happen between tracks when playing cue format.
2. Rectified the bug that the albums from a specified artist are placed into one album.



Instruction For Firmware update:
1. Extract the zip file and copy the update.img onto a micro SD card root folder.
2. Insert the micro SD card into the SD card slot2. Make sure there is no Micro SD card placed in Slot 1.
3. Select Settings¡úAdvanced¡úSystem update (the system update option 
    appears only after the update.img is detected).
4. Click ¡°OK¡± to start the firmware update.
5. The DX120 will reboot after the firmware update is completed.
6. Select Settings¡úAdvanced¡úFactory Reset to reset the DX120. 
    This is to avoid conflicts with residual settings from the previous firmware.
7. Delete the update.img from the micro SD card.